I will want to probably use the midpoint between the two control points for the induced angle of attack.

Get surface out of System. Ie do System.surfaces or induced\_velocity(rcp, system.surfaces[1], system.\Gamma ).

(System.surfaces[1])[i j].rcp will give me the rcp. I must access each panel individually and iterate through all the panels to get the xyz values of each panel.